Welcome to the docs!
Update 1024 of the "Super AUJP" Version 4

I will be making this a breif "How to" for making the bin useable with the users calibration.
If anyone has any comments or suggestions on settings for the MT/IAC stuff let me know and I'll include them.


Blah..., Blah...

Use the difference tool within TunerPro to copy over your specific calibration items.
Use the "Limit" to defined items when first doing the compare to reduce the number of items.

Using the "Copy from Compare" in the toolbox and constant editor, you'll have your specific settings transferred in no time.
Items AFTER address 8824 are specific to the V4 bin and code and should be left alone when doing the compare/transfer.

Add the items shown in the JPG file to your XDF and edit the settings.