## AVR309:USB to UART device installation

### Hardware installation

Your computer must be running Microsoft Windows 98, Windows ME, Windows 2000 or Windows XP.
Under Windows 98
Under Windows XP

Note: The pictures displayed bellow in each step are for AVR309:USB to UART device Advanced version (first picture) and for Simple version (second picture).

Installation steps under Windows 98:

1. Your computer must be switched on and running Microsoft Windows.
2. Connect AVR309:USB to UART device based device to USB port on your computer.
3. "New hardware found" window appears (with "AVR309:USB to UART ..." name).
4. Window "Add New Hardware Wizard" will be opened.
5. Click "Next":
6. Choose "Search for the best driver for your device (Recommended)" and click "Next":
7. Check "Specify location" and "Browse" to the folder where are driver files stored (CD or download folder):
   And then click "Next".
8. In the next window (with founded AVR309:USB to UART protocol converter ...) click "Next":
   Windows then will install necessary driver files and makes system changes. Rebuild of Windows driver database may appears.
9. Installation is complete. Click "Finish" in the last window:
10. Check if the device "AVR309:USB to UART protocol converter ..." is present in "Start - Settings -Control Panel - System - Device Manager - Universal Serial Bus controllers":
11. Device was successfully installed.

Installation steps under Windows XP:

1. Your computer must be switched on and running Microsoft Windows.
2. Connect AVR309:USB to UART ... based device to USB port on your computer and wait.
3. "Found new hardware" window appears (with "AVR309:USB to UART ..." name):
4. Window "Found New Hardware Wizard" will be opened.
   Choose "Install from a list or specify location (Advanced)" and click "Next":
5. Check "Include this location in the search" and "Browse" to the folder where are driver files stored (CD or download folder):
   And then click "Next".
6. The next window (with device AVR309:USB to UART protocol converter ...) appears:
   If warning window "Hardware installation" appears, choose "Continue Anyway":
7. Windows then will install necessary driver files and makes system changes:
8. Installation is complete. Click "Finish":
9. After successful installation the next small window with confirmation of installation appears:
10. Check if the device "AVR309:USB to UART protocol converter ..." is present in "Start - Settings - Control Panel - System - Device Manager - Universal Serial Bus controllers":
11. Device was successfully installed.

Author: Ing. Igor Cesko, Slovakia, www.cesko.host.sk